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SINK DESCRIPTION
 Undermount Single Bowl Kitchen sink
 18 gauge stainless steel 304, Satin finish
 Off-set drain location
 Installation Hardware included
 Proprietary sound absorbing technology that undercoats the surface of this stainless steel kitchen sink keeps it silent and protected from condensation

CUTOUT DIMENSTIONS
Template included, template number HM3117

PRODUCT COMPLIANCE
 All product certified by IAPMO to meet standards ASME A112.19.3/CSA B45.4-17

WARRANTY
[image: ] Limited lifetime warranty against material or manufacturing defects to the original consumer purchaser

TECHNICAL SPECIFICATION

Specification
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	HM-3117
	9”
	Off-set
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	Installation
	Under-mount

	Bowl area
	Length: 32”       (Outside)
14 1/2”	   (Left of Inside)
14 1/2”    (Right of Inside)
Width: 18”	   (Outside)
16”       (Inside)
Bowl Depth: 9”   


	Drain Hole
	4-1/2” 

	
Template
	
Required, Included





















Note:
Install this product according to	the installation instruction Minimum base cabinet size 33”
Consult an installer for confirmation.
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FOR MORE INFORMAITON CALL: 571.393.7576
www.dynamicstonetools.com
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