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SINK DESCRIPTION
 Undermount Single Bowl Kitchen sink
 18 gauge stainless steel 304, Satin finish
 Rear drain location
 Installation Hardware included
 Proprietary sound absorbing technology that undercoats the surface of this stainless steel kitchen sink keeps it silent and protected from condensation

CUTOUT DIMENSTIONS
Template included, template number HM2318ADA

PRODUCT COMPLIANCE
 All product certified by IAPMO to meet standards ASME A112.19.3/CSA B45.4-17

 WARRANTY
 Limited lifetime warranty against material or manufacturing defects to the original consumer purchaser

TECHNICAL SPECIFICATION

SpecificationInstallation
Under-mount
Bowl area
Length: 23” (Outside)
21”	(Inside)
Width: 18”	(Outside)
16”	(Inside)
Bowl Depth: 5-1/2”
Drain Hole
4-1/2” 

Template

Required, Included
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Note:
Install this product according to	the installation instruction Minimum base cabinet size 24”
Consult an installer for confirmation.
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FOR MORE INFORMAITON CALL: 571.393.7576
www.dynamicstonetools.com
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